{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Arkusz1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Arkusz1","index":0,"n_rows":49,"n_cols":5,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["l.p.","Asortyment","wymiary","ilość","producent"]
[]
[1,"Kolano elektrooporowe PE 45' (do zgrzewania)","D 160","1 szt","+GF+"]
[2,"Kolano elektrooporowe PE 90' (do zgrzewania)","D 160","2 szt","+GF+"]
[3,"Kolano PE HD 45'","D 110","2 szt","Geberit"]
[4,"Mufa elektooporowa PE (do zgrzewania elektrycznego)","D 160","3 szt","+GF+"]
[5,"Mufa elektooporowa PE (do zgrzewania elektrycznego)","D 160","4 szt","Geberit"]
[6,"Opaska przyłączeniowa PE z gwintem wewn.","160 x 1 1/2”","3 szt","Astore"]
[7,"Opaska przyłączeniowa PE z gwintem wewn.","160 x 1”","4 szt","Astore"]
[8,"PVC-U Kolano   90'","D 125","2 szt","+GF+"]
[9,"PVC-U Kolano   90'","D 140","2 szt","Astore"]
[10,"PVC-U Kolano   90'","D 160","1 szt","Astore"]
[11,"PVC-U Kolano 90'","D 315","1 szt","Astore"]
[12,"PVC-U Kołnierz","D 315","6 szt","Astore"]
[13,"PVC-U Mufa ","D 160","3 szt","Astore"]
[14,"PVC-U Mufa ","D 140","2 szt","+GF+"]
[15,"PVC-U Mufa ","D 125","2 szt","+GF+"]
[16,"PVC-U Rura ","D 315","2,50m","Astore"]
[17,"PVC-U Trójnik redukcyjny ","160x90x160","8 szt","Astore"]
[18,"PVC-U Trójnik równoprzelotowy","D 315","3 szt","Astore"]
[19,"PVC-U Tuleja kołnierzowa ","D 315","5 szt","Astore"]
[20,"Rura osłonowa karbowana AROT ","D 50","25 m"]
[21,"Rura stalowa K.O.  304L","154 x 2","1,50 m"]
[22,"Rura stalowa K.O.  304L","104 x 2","1,44 m"]
[23,"Rura stalowa K.O.  304L","204 x 2","2,15 m"]
[24,"Uchwyt PE D 315","D315","2 szt","Astore"]
[25]
[26,"Mieszadło gumowane Ø900, dł wału 280cm, 3 łopaty","Ø900","3 szt","MiltonRoy"]
[27]
[28,"Kołnierz luźny aluminiowy PN10","DN 65","8 szt"]
[29,"Kołnierz luźny aluminiowy PN10","DN 80","8 szt"]
[30,"Kołnierz luźny aluminiowy PN10","DN 100","1 szt"]
[31,"Kołnierz luźny aluminiowy PN10","DN 150","4 szt"]
[32,"Kołnierz luźny aluminiowy PN10","DN 200","3 szt"]
[33,"Kołnierz luźny stalowy PN10  1.4307","DN 80","1 szt"]
[34,"Kołnierz luźny stalowy PN10  304L  EN1092-1","DN 200","1 szt"]
[35,"Wywijka  1.4301/07  ","204 x 2","3 szt"]
[36,"Wywijka  1.4301/07  ","159 x 3","4 szt"]
[37,"Wywijka  1.4541","85 x 2","1 szt"]
[38,"Wywijka  316L","104 x 2","1 szt"]
[39,"Kolano stalowe  1.4404","88,9 x 2","4 szt"]
[40,"Kolano stalowe  1.4307","88,9 x 2","4 szt"]
[41,"Kolano stalowe  1.4307","76,1 x 2","6 szt"]
[42]
[43]
[44]
[45]
[46]
[47]